List Industries SUPERIOR( 
Bench Top and Pedestal Specifications
Benchtops:  To be 9-1/2” wide x 1-1/4” thick and made from laminated hardwood. Benchtops are to be finished with one coat deep penetrating sealer and two coats of heavy body high impact hot hydraulically applied lacquer. Benches up to 8’-0” in length have two pedestals.  Benchtops longer than    8’-0” up to 12’-0” are supplied with three pedestals. 
No. 4805 Heavy-Duty Steel Pedestal:  Fabricated from 1-1/2” diameter 14 gauge steel tube welded to top and bottom 11 gauge formed flanges.  Each flange to have three anchoring holes.  Color: #729 Tan. 
No. 4810 Extra Heavy-Duty Cast-Iron Pedestal:  One-piece cast-iron pedestal to include 6” diameter top and bottom flanges.  Each flange to have three anchoring holes. Multiple pieces constructed pedestal are not acceptable.  Color #729 Tan. 
No. 4820 Standard Moveable Pedestal: Fabricated of extruded aluminum providing four anchoring holes at bottom.  Pedestal is designed to be moveable type if desired.  Color #729 Tan. 
No. 4830 Stainless Steel Pedestal: Fabricated from 14 gauge stainless steel.  Pedestal is designed to be moveable but includes 4 holes for anchoring to floor if desired.  Unpainted 
No. 8032 Pedestal: Adjustable height pedestal consisting of a cast aluminum base, threaded pipe nipple and steel pipe flange at the top.  Anchoring through the cast aluminum base is concealed.   Color #729 Tan.
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